CI-110 Installation Instructions
1 July 2005


The CI-110 Plant Canopy Digital Imager can be installed on Windows 2000 and Windows XP computers.

Insert the CD and if autorun is enabled, the Setup.exe program will automatically start.  If autorun is disabled, open My Computer, select the CD drive, and double click on Setup.exe.  The CI-110.exe program will be installed in the C:\Program Files\CI-110 directory unless you tell it to do otherwise.

Plug the instrument into the computer's USB port.  A New Hardware Found wizard should start.  

For Windows 2000:

Select Next

Select Search for a suitable driver for my device (recommended)

Select only Specify a location
 
Browse to the CD directory Win2000 and select OK

Select Next

When it asks if you want to Continue the installation, select Yes

Select Finish

Do the same for the next part of the composite USB device found.






For Windows XP:

Select "No, not this time" when it asks to connect to Windows Update.

Select "Install from a list or specific location (Advanced).

Select only the "Include this location in the search" and browse to the CD dirctory WinXP.
The computer should find the Belkin USB VideoBuss II, Video installation package and ask to Continue Anyway (software has not passed Windows Logo testing).  Select Continue Anyway.

Select Finish

The New Hardware Wizard should launch again for the Belkin VideoBus II Audio. Follow the same instruction for it:
Select No, not this time.
Install from a list or specific location.
Include this location in the search: D:\WinXP (use the drive letter for your CD drive)
Continue Anyway
Finish



